Activate service mode according to: DIAGNOSTICS/VEHICLE COMMUNICATION/Advanced/PBM/Activating and service

Remove rear wheel



Warning! Make sure that no load is placed on the brake hose.

Torque: Slide rail rear brake caliper, 35 Nm



**Note!** Make sure that the correct side of the tool (flat side) is facing the brake piston. The brake piston must be pushed in, not rotated.

Installation



**Note!** Make sure that the mating faces are clean and free of foreign material.

Use: Silicone grease, 1161688

To install, reverse the removal procedure.

Deactivate service mode according to: DIAGNOSTICS/VEHICLE COMMUNICATION/Advanced/PBM/Activating and service

DISK

With car jacked and wheel off and service mode on EPB



Warning! Make sure that no load is placed on the brake hose.

Torque: Mount rear brake caliper, 110 Nm



Torque: Rear brake disc to wheel hub, 35 Nm



Installation

To install, reverse the removal procedure.

Perform parking brake, adjusting - Deactivate service mode according to: DIAGNOSTICS/VEHICLE COMMUNICATION/Advanced/PBM/Activating and service